**Section 1328.305 Wireless Carrier Testing**

a) No circuits associated with an authorized wireless 9-1-1 answering point shall be opened, grounded, short circuited or tested in any manner until maintenance personnel have obtained release of the affected circuits from the appropriate 9-1-1 authority. Wireless carrier maintenance personnel shall advise the 9-1-1 authority regarding the length of time that will be required to perform any work involving circuits associated with an authorized wireless 9-1-1 answering point. Wireless carrier personnel shall notify the 9-1-1 authority and the 9-1-1 system provider a minimum of 48 hours prior to performing mobile office switching installations, NPA additions, NXX additions, or any other scheduled event that affects 9-1-1.

b) Each wireless carrier shall adopt mutually agreed upon testing practices, in conjunction with the 9-1-1 authority, to perform, at a minimum, mobile office to PSAP 9-1-1 test calls when any of the following changes occur:

1) New mobile switching office installations;

2) NPA and NXX pANI additions;

3) Local number portability implementations;

4) Number pooling implementations; and

5) Any other event that affects 9-1-1.

c) Each wireless carrier shall develop a testing plan in conjunction with the 9-1-1 system provider and the 9-1-1 authority for inclusion in the 9-1-1 systems' wireless plan that must be submitted to the Administrator.