**Section 3700.75 Special Provisions for Levees and Floodwalls**

The flood discharge that would just overtop a levee or floodwall shall be used for the worst-case analysis (see Section 3700.20).

(Source: Amended at 38 Ill. Reg. 934, effective December 27, 2013)