**Section 336.50 Community Water Supply Testing Categories**

For the purposes of this Part, the following testing categories shall initially be assigned to community water supplies based on drinking water testing results on file at IEPA as of November 16, 2007.

|  |  |
| --- | --- |
| Category | Service |
| 4109 | Gross alpha analysis |
| 4006 | Total uranium analysis |
| 4010 | Radium-226 and radium-228 analysis |
| RDS | Gross alpha, radium-226 and radium-228 analysis |
| RDU | Gross alpha, radium-226, radium-228 and total uranium analysis |

AGENCY NOTE: If gross alpha result is greater than 15 pCi/L, IEPA requires an additional total uranium analysis (4006).

(Source: Amended at 32 Ill. Reg. 2585, effective February 4, 2008)