**Section 211.450 Airless Spray**

"Airless spray" means a spray coating method in which the coating is atomized by forcing it through a small opening at high pressure. The coating liquid is not mixed with air before exiting from the nozzle.

(Source: Added at 17 Ill. Reg. 16504, effective September 27, 1993)