**Section 212.450 Liquid Steel Charging**

Particulate matter emissions from liquid steel charging in continuous casting operations shall be controlled by chemical or mechanical shrouds or methods of comparable effectiveness.

(Source: Amended at 3 Ill. Reg. 39, p. 184, effective September 28, 1979)