**Section 214.423 Slab Reheat Furnaces in St. Louis Area**

Section 214.304 notwithstanding, slab reheat furnaces in the St. Louis (Illinois) major metropolitan area with fuel burning capacities in excess of 650 mmbtu/hr and burning any residual fuel shall not be subject to the applicable Subpart B through F so long as the total sulfur dioxide emissions resulting from the burning of residual fuel oil in all such furnaces at any one steel mill do not exceed 730 lbs/hr.

(Source: Adopted at 7 Ill. Reg. 4219, effective March 28, 1983)