**Section 216.101 Measurement Methods**

Carbon Monoxide concentrations in an effluent stream shall be measured by the non-dispersive infrared method or by other methods approved by the Illinois Environmental Protection Agency (Agency) according to the provisions of 35 Ill. Adm. Code 201.