**Section 241.APPENDIX B Credit Values**

**TABLE A Credit Generation: Acquiring a Light-Duty Clean Fuel Vehicle before MY 1999 or Acquiring More Light-Duty Clean Fuel Vehicles than Required**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |
| TYPE | LDV, LDT  <6000 GVWR  <3750 LVW | LDT <6000  GVWR >3750  VLW<5750  LVW | LDT >6000  GVWR <3750  ALVW | LDT >6000  GVWR >3750  ALVW <5750  ALVW | LDT >6000  GVWR >5750  ALVW |
| LEV | 1.00 | 1.26 | 0.71 | 0.91 | 1.11 |
| ULEV | 1.20 | 1.54 | 1.00 | 1.26 | 1.56 |
| ZEV | 1.43 | 1.83 | 1.43 | 1.83 | 2.23 |

(Source: Amended at 21 Ill. Reg. 15767, effective November 25, 1997)

**TABLE B: Credit Generation: Acquiring Light-Duty ULEV or ZEV Clean Fuel Vehicles**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |
| TYPE | LDV, LDT  <6000 GVWR  <3750 LVW | LDT < 6000  GVWR  > 3750 LVW  < 5750 LVW | LDT >6000  GVWR  <3750 ALVW | LDT >6000  GVWR  >3750 ALVW <5750 ALVW | LDT >6000  GVWR >5750  ALVW |
| ULEV | 0.20 | 0.29 | 0.29 | 0.34 | 0.45 |
| ZEV | 0.43 | 0.57 | 0.71 | 0.91 | 1.11 |

**TABLE C: Credits Needed in Lieu of Acquiring a Light-Duty LEV**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |
| TYPE | LDV, LDT  <6000 GVWR  <3750 LVW | LDT < 6000  GVWR  > 3750 LVW  < 5750 LVW | LDT >6000  GVWR  <3750 ALVW | LDT >6000  GVWR  >3750 ALVW <5750 ALVW | LDT >6000  GVWR  >5750  ALVW |
| LEV | 1.00 | 1.26 | 0.71 | 0.91 | 1.11 |

**TABLE D Credit Generation: Acquiring a Heavy-Duty Clean Fuel Vehicle before MY 1999 or Acquiring More Heavy-Duty Clean Fuel Vehicles than Required**

|  |  |
| --- | --- |
| VEHICLE TYPE | HDV |
| LEV | 1.00 |
| ULEV | 1.87 |
| ZEV | 3.53 |

(Source: Amended at 21 Ill. Reg. 15767, effective November 25, 1997)

**TABLE E: Credit Generation: Acquiring Heavy-Duty ULEV or ZEV Clean Fuel Vehicles**

|  |  |
| --- | --- |
| VEHICLE TYPE | HDV |
| ULEV | 0.87 |
| ZEV | 2.53 |

**TABLE F: Credits Needed in Lieu of Acquiring a Heavy-Duty LEV**

|  |  |
| --- | --- |
| VEHICLE TYPE | HDV |
| LEV | 1.00 |