**Section 266.145 Process Weight Rate for Inoculation, Demagging, Degassing**

The process weight rate for inoculation, demagging, degassing and related operations is calculated by using the weight of the material added to the bath.