**Section 266.155 Process Weight Rate for Shakeout Operations**

The process weight rate for shakeout operations is calculated by using the weight of the sand and other materials freed from the casting.