**Section 266.160 Process Weight Rate for Drying Operations**

The process weight rate for drying operations is calculated by using the weight of the material to be dried, as weighed entering the dryer.