**Section 266.180 Process Weight Rate for Quenching**

The process weight rate for quenching is calculated by using the weight of the quench material added to the bath.