**Section 266.185 Process Weight Rate for Scarfing Operations**

The process weight rate for scarfing operations is calculated by using the weight of all material removed by scarfing.