**Section 370.1080 Sampling and Testing**

a) Facilities shall be included for collecting samples, as monitoring requirements warrant, of the disinfected effluent.

b) Where chlorine disinfection is used, equipment shall be provided for measuring chlorine residual using accepted test procedures.

c) Where required by the Agency, equipment shall also be provided for measuring fecal coliform using accepted test procedures.

(Source: Amended at 21 Ill. Reg. 12444, effective August 28, 1997)