**Section 406.108 Non-Point Source Mine Discharges**

Surface drainage from the affected land of a coal mine, including disturbed areas that have been graded, seeded, or planted, must pass through a sedimentation pond or a series of sedimentation ponds before leaving the facility.

(Source: Amended at 43 Ill. Reg. 11620, effective September 25, 2019)