**Section 611.TABLE D Number of Lead and Copper Monitoring Sites**

|  |  |  |
| --- | --- | --- |
| System Size (Persons Served) | Number of Sites  (Standard Monitoring) | Number of Sites  (Reduced Monitoring) |
| More than 100,000 | 100 | 50 |
| 10,001-100,000 | 60 | 30 |
| 3,301 to 10,000 | 40 | 20 |
| 501 to 3,300 | 20 | 10 |
| 101 to 500 | 10 | 5 |
| 100 or fewer | 5 | 5 |

BOARD NOTE: Derived from 40 CFR 141.86(c) (2012).

(Source: Amended at 37 Ill. Reg. 1978, effective February 4, 2013)