**Section 615.463 Design and Operating Requirements**

This Section applies six months after the date of first applicability to a waste pile not subject to Section 615.462,

a) The owner or operator must not cause or allow:

1) Disposal or storage in the waste pile of liquids or materials containing free liquids; or

2) Migration and runoff of leachate into adjacent soil, surface water, or groundwater.

b) The waste pile must comply with the following standards:

1) The waste pile must be under an impermeable membrane or cover that provides protection from precipitation;

2) The waste pile must be protected from surface water run-on; and

3) The waste pile must be designed and operated to control wind dispersal of waste by a means other than wetting.

(Source: Amended at 47 Ill. Reg. 7581, effective May 16, 2023)