**Section 725.360 Monitoring and Inspections**

An owner or operator required to have a LDS under Section 725.354 must record the amount of liquids removed from each LDS sump at least once each week during the active life and closure period.

(Source: Amended at 29 Ill. Reg. 6389, effective April 22, 2005)