**Section 726.APPENDIX K Lead-Bearing Materials that May be Processed in Exempt Lead Smelters**

a) Exempt lead-bearing materials when generated or originally produced by lead-associated industries.

 BOARD NOTE: Lead-associated industries are lead smelters, lead-acid battery manufacturing and lead chemical manufacturing (e.g., manufacturing of lead oxide or other lead compounds).

 Acid dump/fill solids

 Sump mud

 Materials from laboratory analyses

 Acid filters

 Baghouse bags

 Clothing (e.g., coveralls, aprons, shoes, hats, gloves)

 Sweepings

 Air filter bags and cartridges

 Respiratory cartridge filters

 Shop abrasive

 Stacking boards

 Waste shipping containers (e.g., cartons, bags, drums, cardboard)

 Paper hand towels

 Wiping rags and sponges

 Contaminated pallets

 Water treatment sludges, filter cakes, residues, and solids

 Emission control dusts, sludges, filter cakes, residues, and solids from lead-associated industries (e.g., K069 and D008 wastes)

 Spent grinds, posts and separators

 Spend batteries

 Lead oxide and lead oxide residues

 Lead plates and groups

 Spent battery cases, covers, and vents

 Pasting belts

 Water filter media

 Cheesecloth from pasting rollers

 Pasting additive bags

 Asphalt paving materials

b) Exempt lead-bearing materials when generated or originally produced by any industry.

 Charging jumpers and clips

 Platen abrasive

 Fluff from lead wire and cable casings

 Lead-based pigments and compounding pigment dust

(Source: Amended at 37 Ill. Reg. 3249, effective March 4, 2013)