**Section 726.APPENDIX K Lead-Bearing Materials that May be Processed in Exempt Lead Smelters**

a) Exempt lead-bearing materials when generated or originally produced by lead-associated industries.

BOARD NOTE: Lead-associated industries are lead smelters, lead-acid battery manufacturing and lead chemical manufacturing (e.g., manufacturing of lead oxide or other lead compounds).

Acid dump/fill solids

Sump mud

Materials from laboratory analyses

Acid filters

Baghouse bags

Clothing (e.g., coveralls, aprons, shoes, hats, gloves)

Sweepings

Air filter bags and cartridges

Respiratory cartridge filters

Shop abrasive

Stacking boards

Waste shipping containers (e.g., cartons, bags, drums, cardboard)

Paper hand towels

Wiping rags and sponges

Contaminated pallets

Water treatment sludges, filter cakes, residues, and solids

Emission control dusts, sludges, filter cakes, residues, and solids from lead-associated industries (e.g., K069 and D008 wastes)

Spent grinds, posts and separators

Spend batteries

Lead oxide and lead oxide residues

Lead plates and groups

Spent battery cases, covers, and vents

Pasting belts

Water filter media

Cheesecloth from pasting rollers

Pasting additive bags

Asphalt paving materials

b) Exempt lead-bearing materials when generated or originally produced by any industry.

Charging jumpers and clips

Platen abrasive

Fluff from lead wire and cable casings

Lead-based pigments and compounding pigment dust

(Source: Amended at 37 Ill. Reg. 3249, effective March 4, 2013)