**Section 742.315 Soil Ingestion Exposure Route**

The soil ingestion exposure route may be excluded from consideration if:

a) The requirements of Sections 742.300 and 742.305 are met;

b) An approved engineered barrier is in place that meets the requirements of Subpart K;

c) Safety precautions for the construction worker are taken if the Tier 1 construction worker remediation objectives are exceeded; and

d) An institutional control, in accordance with Subpart J, will be placed on the property.

(Source: Amended at 25 Ill. Reg. 10374, effective August 15, 2001)