**Section 814.902 Standards for Operation and Closure**

a) All units regulated in this Subpart I are subject to all requirements in Subpart C of 35 Ill. Adm. Code 817.

b) If an owner or operator of a unit regulated under this Subpart I is unable to obtain the representative leachate samples required pursuant to 35 Ill. Adm. Code 817.305(a), representative core samples must be taken at appropriate locations in the unit. Each sample must be individually subjected to the ASTM Method D3987-85 extraction procedure, incorporated by reference in 35 Ill. Adm. Code 810.104. The resulting leachate from the extraction procedure must be substituted for that to be collected pursuant to 35 Ill. Adm. Code 817.305(a).

(Source: Amended at 38 Ill. Reg. 7294, effective March 13, 2014)