**Section 160.490 Fire Extinguishers**

Each tank truck or tank wagon shall carry a fire extinguisher suitable for extinguishing gasoline and oil fires, such as carbon dioxide, foam or powder. Such fire extinguishers shall carry a testing and listing label giving the extinguisher a rating for class A & B fires.

(Source: Amended at 9 Ill. Reg. 10012, effective October 1, 1985)