**Section 330.3410 Fire Alarm and Detection System**

a) There shall be an approved fire detection and alarm system throughout the facility. (A, B)

b) The fire alarm system shall be manually and automatically operated, electrically supervised, and be equipped with automatic detectors. Pre-signal systems are not permitted. (A, B)

c) The system shall automatically transmit the alarm to any available municipal fire department by direct private lines or through an approved central station. (A, B)

d) The fire alarm system shall be tested at least weekly. (A, B)

(Source: Amended at 13 Ill. Reg. 6562, effective April 17, 1989)