**Section 750.1680 Floors**

Floors shall be made of concrete, tight wood, asphalt, or other similar cleanable material, except that dirt or gravel floors may be used if graded to preclude the accumulation of liquids and covered with removable, cleanable platforms or duckboards.