**Section 785.512 Equipment and Utensils − General Construction, Repair, and Installation**

All equipment and utensils necessary to the manufacture of dry milk products, including pasteurizer, timing pump or device, flow diversion valve and recorder controller, shall meet the same general requirements as outlined in Section 785.415. In addition, for certain other equipment the following requirements shall be met.