**Section 785.554 Filler and Packaging Equipment**

All filling and packaging equipment shall be of sanitary construction and all parts, including valves and filler heads, accessible for cleaning in accordance with 3-A Sanitary Standards.