**Section 890.670 Strainers and Fixture Outlets**

a) Strainers. All plumbing fixtures other than water closets, urinals with integral traps, and any sink outlet having a disposal unit shall be provided with a strainer. A pop-up waste shall be considered a strainer.

b) Bathtubs − Waste Outlets. The waste outlet for a bathtub shall have a strainer or stopper and shall have an outlet at least one and one-half (1 ½) inches in diameter.