**Section 890.800 Special Fixtures and/or Items Designed for a Particular Purpose**

a) Emergency showers and eye wash stations within a building shall be provided with potable water and a trapped and vented receptor and shall comply with ANSI Z358.1.

b) Emergency eye wash stations shall not be installed on a faucet spout.

c) Baptistries, ornamental and lily ponds, aquariums, ornamental fountain basins, and similar type constructions, when provided with water supplied from the potable water system, shall be protected from back siphonage as required in Section 890.1130(f).

d) A request for permission to install special fixtures or items designed for a particular purpose requiring water and waste connections not otherwise provided for in this Part shall be submitted, in writing, to the Department for approval prior to installation.

(Source: Amended at 38 Ill. Reg. 9940, effective April 24, 2014)