**Section 460.380 Installation Inspections**

Within 90 days after installation or exchange of any meter with associated instrument transformers and/or phase-shifting transformers, a post-installation inspection shall be made under load to determine if the meter is accurately measuring customer energy consumption.