**Section 442.305 Ventilation**

The body shall be equipped with a suitable controlled ventilation system of sufficient capacity to maintain a satisfactory ratio of outside to inside air under operating conditions without opening of windows except in warm weather.